**Technical specifications**

|  |  |
| --- | --- |
| **Print width (up to)** | 106mm for ALX 734 127mm for ALX 735 160mm for ALX 736 |
| **Print speed (up to)** | 400mm/s for ALX 734 300mm/s for ALX 735/6 |
| **Dispensing speed (up to)** | Up to 50m/min for all models |
| **Printing technology** | Thermal transfer/direct thermal |
| **Print head** | 300 dpi near edge or print head |
| **Ribbon save** | Yes: Automatic head-lift |
| **Ribbon length** | Up to 1,000m |
| **Graphic formats** | BMP, PCW, JPG, TIF, GIF, Easy Plug Logos |
| **Label output** | Up to 400 labels/min |
| **Maximum label width** | 134mm for ALX 734 & ALX 735 185mm for ALX 736 |
| **Maximum label length** | 225mm – up to 440mm after elongation dispense edge fixture |